|  |  |
| --- | --- |
| **Наименование параметра, единица измерения** | **ИРТП2-240, ИРТП4-240** |
| норма | данные испытаний |
| не менее | номинал | не более |
| Амплитуда импульсного напряжения на трубке, кВ | 180 | 210 | 240 |   |
| Диаметр фокусного пятна, мм | - | 3 ± 0.5 | - | 3 ± 0.5 |
| Экспозиционная   доза   рентгеновскою   излучения за   стальной   преградой толщиной 40 мм, Р (при напряжении на трубке 240 кВ на расстоянии 21 см от окна трубки и выходной емкости источника питания трубки 50 пФ) | 30 х 10-3 | - | - | (40-50) х 10-3 |
| Гарантийная наработка (в пределах гарантийного срока), имп. |   | 106 |   | 106 |
| Габариты, d х l, мм |   | 62 х 136, 62 x 122 |   |   |
| Масса, кг, не более |   | 0.35 |   |   |
| ***Параметры режима измерений*** |
| Емкость, разряжаемая на трубку, пФ | - | 50 | - |   |
| Частота следования рентгеновских вспышек, Гц | - | 10 | - |   |
| Время экспозиции, с | - | 60 ± 1 |   |   |

|  |  |
| --- | --- |
| **Characteristic, unit measure** | **IRTP2-240, IRTP4-240** |
| rate | test data |
| min | nominal | max |
| Pulse voltage amplitude, kv | 180 | 210 | 240 |   |
| Focus spot diameter, mm | - | 3 ± 0.5 | - | 3 ± 0.5 |
| X-ray radiation exposure doze behind the steel barrier of 40 mm | 30 И 10-3 | - | - | (40-50) И 10-3 |
| Warranty operation time, pulses |   | 106 |   | 106 |
| Size, d x l, mm |   | 62 И 136, 62 x 122 |   |   |
| Mass, kg, max |   | 0.35 |   |   |
| ***Characteristic of measurement mode*** |
| Capacity discharge on the tube, pf | - | 50 | - |   |
| X-ray flares' repetition rate, Hz | - | 10 | - |   |
| Exposure time, sec | - | 60 ± 1 |   |   |