**Технические характеристики сеялок СОНП:**

|  |  |  |
| --- | --- | --- |
|  | **СОНП-4,2** | **СОНП-2,8** |
| Тип сеялки | навесная |
| Ширина захвата, м | 4,2 | 2,8 |
| Производительность за час основного времени, га/ч  | 3,36 | 2,1 |
| Количество высевающих секций | от 6 до 12 | от 4 до 8 |
| Глубина заделки семян, мм | 20-50 |
| Ширина междурядий, мм | от 200 | от 250 |
| Емкость бункера, дм3 | до 8 |
| Тип сошников | полозовидные однострочные, двухстрочные |
| Габаритные размеры, мм (ДхШхВ): |
|        · в рабочем положении | 2300 х 6000 | 2200 х 3300 |
|        · в транспортном положении | 6000 х 2300 х 2500 | 2200 х 3300 |
| Рабочая скорость, км/ч | от 3 до 8 |

**Technical characteristics of seeders SONP:**

|  |  |  |
| --- | --- | --- |
|  | **SONP-4.2** | **SONP-2.8** |
| Type of seeder | mounted |
| Grasp width, m | 4,2 | 2,8 |
| Productivity per hour of regular time, ha/h  | 3,36 | 2,1 |
| Number of sowing sections | from 6 to 12 | from 4 to 8 |
| Depth of seeding, mm | 20-50 |
| Row-spacing width, mm | from 200 | from 250 |
| Tank capacity, dm3 | up to 8 |
| Plowshares type | runner type, one-row, two-row |
| Overall dimensions (LхWхH), mm: |
|        · in operating position | 2300 х 6000 | 2200 х 3300 |
|        · in transport position | 6000 х 2300 х 2500 | 2200 х 3300 |
| Operating speed, km/h | from 3 to 8 |