| NAME | 32552-5013-71 | 3255-5013-71-28 | 32551-5013-71 |
| --- | --- | --- | --- |
| Wheel arrangement | 4x4 | 6x6 | 6x6 |
| Seating capacity in wagon body | 20 | 22\* | 20 |
| Kerb weight, kg | 9550 | 11960 | 10475 |
| Gross vehicle weight, kg | 13300 | 13300 | 13300 |
| GVW distribution, kg: | on front axle: 5300 on rear axle: 8000 | on front axle: 5300 on rear axle: 8000 | on front axle: 5300 on rear axle: 8000 |
| Max travelling speed, km/h | 85 | 85 | 85 |
| Engine: | YMZ-53622-10, in-line, (Emission class-4) | YMZ-53622-10, in-line, (Emission class-4) | YMZ-53622-10, in-line, (Emission class-4) |
| rated power, hp | 240 | 240 | 240 |
| maximum engine speed, min-1 | 2300 | 2300 | 2 300 |
| maximum torque, kgf-m | 92 | 92 | 92 |
| engine speed at maximum torque, min-1м | 1 300..1 600 | 1 300..1 600 | 1 300..1 600 |
| Gearbox | YMZ-0905 - mechanical, 5-speed | YMZ-0905 - mechanical, 5-speed | YMZ-0905 - mechanical, 5-speed |
| Transfer box | «URAL» Automobile works» JSC, 2-speed, with inter-axle locking differential (high gear - 1,04; low gear - 2,15) | «URAL» Automobile works» JSC, 2-speed, with inter-axle locking differential (high gear - 1,04; low gear - 2,15) | «URAL» Automobile works» JSC, 2-speed, with inter-axle locking differential (high gear - 1,04; low gear - 2,15) |
| Cab | Behind engine, three-seat | Behind engine, three-seat | Behind engine, three-seat |
| Driving axles | «URAL» Automobile works» JSC, axle ratio - 6,77 | «URAL» Automobile works» JSC, axle ratio - 7,49 | «URAL» Automobile works» JSC, axle ratio - 7,49 |
| Fuel tank capacity, l | 300 | 300 | 300 |
| Wheels and tires | Wheels - 533-310, tires - 425/85R21 | Wheels - 515-254, tires - 14.00-20 | Wheels - 515-254, tires - 14.00-20 |
| Overall truck dimensions, mm | 8985x2500x3400 | 10430x2500x3400 | 8985x2500x3400 |