| NAME |  32552-5013-71 |  3255-5013-71-28 |  32551-5013-71 |
| --- | --- | --- | --- |
| Wheel arrangement |  4x4 |  6x6 |  6x6 |
| Seating capacity in wagon body |  20 |  22\* |  20 |
| Kerb weight, kg |  9550 |  11960 |  10475 |
| Gross vehicle weight, kg |  13300 |  13300 |  13300 |
| GVW distribution, kg: |  on front axle: 5300on rear axle: 8000 |  on front axle: 5300on rear axle: 8000 |  on front axle: 5300on rear axle: 8000 |
| Max travelling speed, km/h |  85 |  85 |  85 |
| Engine: |  YMZ-53622-10, in-line, (Emission class-4) |  YMZ-53622-10, in-line, (Emission class-4) |  YMZ-53622-10, in-line, (Emission class-4) |
| rated power, hp |  240 |  240 |  240 |
| maximum engine speed, min-1 |  2300 |  2300 |  2 300 |
| maximum torque, kgf-m |  92 |  92 |  92 |
| engine speed at maximum torque, min-1м |  1 300..1 600 |  1 300..1 600 |  1 300..1 600 |
| Gearbox |  YMZ-0905 - mechanical, 5-speed |  YMZ-0905 - mechanical, 5-speed |  YMZ-0905 - mechanical, 5-speed |
| Transfer box |  «URAL» Automobile works» JSC, 2-speed, with inter-axle locking differential (high gear - 1,04; low gear - 2,15) |  «URAL» Automobile works» JSC, 2-speed, with inter-axle locking differential (high gear - 1,04; low gear - 2,15) |  «URAL» Automobile works» JSC, 2-speed, with inter-axle locking differential (high gear - 1,04; low gear - 2,15) |
| Cab |  Behind engine, three-seat |  Behind engine, three-seat |  Behind engine, three-seat |
| Driving axles |  «URAL» Automobile works» JSC, axle ratio - 6,77 |  «URAL» Automobile works» JSC, axle ratio - 7,49 |  «URAL» Automobile works» JSC, axle ratio - 7,49 |
| Fuel tank capacity, l |  300 |  300 |  300 |
| Wheels and tires |  Wheels - 533-310, tires - 425/85R21 |  Wheels - 515-254, tires - 14.00-20 |  Wheels - 515-254, tires - 14.00-20 |
| Overall truck dimensions, mm |  8985x2500x3400 |  10430x2500x3400 |  8985x2500x3400 |