|  |  |  |
| --- | --- | --- |
| **Parameter, unit** | **Rate, not less** | **Норма, не более** |
| Power consumption, W | — | 30 |
| Power supply, V | 22 | 33 |
| Range of measured angular velocity, ° / s | -1000 | 1000 |
| Gyro zero drift on all axes, ° / h |  |  |
| without calibration | 1 | 2 |
| with calibration duration 5 min | 0,5 | 0,8 |
| with calibration duration 10 min | 0,2 | 0,4 |
| Scale factor (discrete) of the gyroscope, ang.s / imp | 4,3 | 4,5 |
| Instability and non-reproducibility of the scale factor of the gyroscope, relative units | — | 5\*10-4 |
| Operating temperature range, ° С | -55 | +65 |
| Dimensions, mm |  |  |
| diameter | — | 164 |
| height | — | 110 |
| Weight, kg | — | 3,7 |
| Assigned resource, h | 1200 | — |
| Assigned service life, years | 12 | — |