|  |  |
| --- | --- |
| Параметры | Значение |
| **ДГ-880Л** | **ДГ-882Л** | **ДГ-1400** |
| Дизель | 8ДМ-21Л | 8ДМ-21Л2 | 12ДМ-21Л2 |
| Генератор тяговый | ГС-523МУХЛ2 | Агрегат тяговый А724У2 | ГСТ 1400-1500УХЛ2 |
| Род тока | Переменный |
| Номинальная мощность на клеммах, кВт (л.с.) | 880 (1196) | 882 (1200) | 1200 (1632) |
| Продолжительный выпрямленный ток, А | 3600 | 6400 |
| Частота вращения ротора генератора, об/мин. | 1500 | 1500 |
| Габариты, мм: длина, ширина, высота | 5156×1614×1974 | 4804×1560×2243 | 5830×1660×2305 |
| Масса с оборудованием, кг | 12500±50 | 14300 | 16120 |
| Удельный расход топлива г/л.с.ч. | 162+8 | 163+7 | 162+8 |
| Удельный расход масла на угар г/л.с.ч. | 0,84 |

**Characteristics:**

|  |  |
| --- | --- |
| Parameters | Value |
| DG-880L | DG-882L | DG-1400 |
| Diesel motor | 8DM-21EL | 8DM-21EL2 | 12DM-21EL2 |
| Traction generator | GS-523MUHL2 | Locomotive unit A724U2 | GST 1400-1500UHL2 |
| Current type | Alternating current |
| Rated power at the terminals, kW (hp) | 880 (1,196) | 882 (1,200) | 1,400 (1,632) |
| Continuous rectified current, A | 3,600 | 6,400 |
| Rectified pick-up current, A | 5,000 |   |
| Maximum rectified voltage, V | 510 |   |
| Generator rotor speed, rpm | 1,500 | 1,500 |
| Overall dimensions, mm: length, width, height | 5,156×1,614×1,974 | 4,804×1,560×2,243 | 5,830×1,660×2,305 |
| Equipped weight, kg | 12,500±50 | 14,300 | 16,120 |
| Specific fuel consumption, g/hp\*h | 162+8 | 163+7 | 162+8 |
| Specific burning oil consumption, g/hp\*h | 0.84 |