|  |  |  |
| --- | --- | --- |
| **SPECIFICATIONS** | | |
|  | **PI-360CV1** | **PI-600CV1** |
| Screen diameter, mm | 260 | 600 |
| Magnification | 10; 20; 50; 100; 200; 500 | 10; 20; 50; 100; 200 |
| **Measuring stage travel, mm:** |  |  |
| longitudinal direction | 50 | 150 |
| transverse direction | 25 | 75 |
| vertical direction | 85 | 90 |
| Resolution, mm | 0.001 | 0.001 |
| Distortion, mm | ± 0.2 | ± 0.2 |
| Overall dimensions, mm | 700 х 800 х 1600 | 1700 х 2075 х 1950 |
| Weight, kg | 150 | 600 |